# all

The keyword is used in conjunction with other keywords to refer to each entity concerned . It is used to...

1. clear all ports ( together with the keyword clear);
2. start all ports (together with the keyword start);
3. stop all timers, components or ports ( together with the keyword stop);
4. to denote that all definitions must be imported from the source module (together with the keyword import) ;
5. check all parallel components (together with the keyword running);
6. check whether all parallel components have finished execution (together with the keyword done).

Related keywords:

- clear
- done
- import
- running
- start
- stop

### all...

BNF definition of all